Type: Welded Bellows
Stroke: 1.15"
Bellows material: 347 Stainless Steel
Flange material: 304 Stainless Steel
Bellows O.D: 1-1/4"
Bellows I.D: 3/4"
Flange O.D 1: 1-3/8"
Flange O.D 2: 1-3/8"
Leak rate not to exceed 2 X 10-9 STD CC/SEC He.
Pressure: VAC Ext, 1 ATM int.
Max. Temp: 260oC. (500oF).
Life cycle is 10K.
Angular Deflection: 22o
Package individually in heat sealed plastic bags.
Manufacture in accordance with MDC ES0031.