Flange Size: DN 50 ISO-KF
Type: Flexible Coupling
ID: 1-5/8"
Length: 4.220"
Weight: 0.560 lbs
Hose Material: 316 or 321 SS
Flange & Cuff Material: 304 SS
Vacuum Range: Elastomer Seal (HV): > 1 x 10ˉ ⁸ mbar to 1 bar
Metal Seal (UHV): > 1 x 10ˉ¹⁰ mbar to 1 bar
Temperature Range: Elastomer Seal (HV): -20°C to 150°C
Metal Seal (UHV): -200°C to 300°C