Flange Size: DN 25 ISO-KF
Tee Type: Standard Tee
Material: 304 Stainless
Tube OD: 1"
Port Length: 2.040"
Vacuum Range: FKM: 1 · 10-8 mbar to 1 bar
Metal seal: 1 · 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 0.520 lbs