Tee Type: Reducing Tee
Flange Size 1: DN 40 ISO-KF - Tube OD 1: 1-1/2" - Port Length 1: 2.459"
Flange Size 2: DN 16 ISO-KF - Tube OD 2: 3/4" -  Port Length 2: 2.750"
Material: 304 Stainless Steel
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 0.710 lbs