Flange 1: DN 40 CF (2.75" OD)
Type: Straight Reducer
Flange 2: NW 25 (1.57" OD)
Material: 304 Stainless
Bolt Holes (large flange): 6 ea. at 0.265"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 0.830 lbs