Flange Size: DN 63 CF (4.5" OD)
Alignment: Rotatable
Material: 304 Stainless Steel
Bore: 2.510"
Thickness: 0.750"
Bolt Circle: 3.628"
Bolt Hole Diameter: 0.332"
# Bolt Holes: 8
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 2.130 lbs