Flange Size: DN 16 CF (1.33" OD)
Alignment: Non-rotatable
Material: 304 Stainless
Bore: Blank
Thickness: 0.285"
Bolt Circle: 1.062"
Bolt Hole Diameter: 0.172"
# Bolt Holes: 6
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 0.090 lbs