Flange Size: DN 50 CF (3.370" O.D)
Alignment: Non-rotatable
Material: 304 Stainless Steel
Bore: Blank
Thickness: 0.620"
Bolt Circle: 2.850"
Bolt Hole Diameter: 0.332"
# Bolt Holes: 8
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 1.40 lbs