Flange Size: DN 275 CF (13.25" O.D)
Alignment: Non-rotatable
Material: 304 Stainless Steel
Bore: Blank
Thickness: 1.120"
Bolt Circle: 12.060"
Bolt Hole Dia / Thread: 0.391"
# Bolt Holes: 30
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 41.04 lbs