Flange Type: ConFlat CF Flange (DN100CF 152mm | 6.00" OD)
Alignment: Non-rotatable
Material: 316LN (1.4429 | UNS S31653) Low-Carbon Nitrogen-Enhanced Stainless Steel
Thickness: 0.827"
Bore: 1.559"
Bolt circle diameter: 5.118" / 2.44"
Holes thread: M8 X 1.25
# Bolt holes: 16
Complies with ISO 3669
Vacuum Range: 1 X 10-13 Torr or below 10-13 mbar
Temperature Range: 200oC to 450oC
High temperature rated to 450oC
Compatible with other manufacturers' Conflat® knife-edge flanges
Weight: 4.67 lbs