Flange Size: DN 200 CF (10" OD)
Alignment: Non-rotatable
Material: 304 Stainless Steel
Bore: Blank
Thickness: 0.970"
Bolt Circle: 9.128"
Bolt Hole Thread: 5/16-24 UNF
# Bolt Holes: 24
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 20.60 lbs