Flange: DN 40 CF (2.75" OD)
Type: Half Nipple
Tube OD: 1-1/2"
Material: 304 Stainless
Length: 2.470"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 0.730 lbs