Flange size: DN 16 CF (1.33" OD)
Type: Half Nipple
Material: 304 Stainless
Tube: 3/4" O.D, 0.035" W.
Length: 1.510"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 0.110 lbs