Tube OD: 2.0"
Elbow Type: Radius 90 Degree
Material: 304 Stainless Steel
Port Length: 3.00"
Wall Thickness: 0.065"
Finish: Bead Blast
Vacuum Range: 1 X 10-13 mbar to 1 bar
Temperature Range: -200 °C to 450 °C
Weight: 0.540 lbs