Flange: DN 40 CF (2.75" OD)
Type: Full Nipple
Material: 304 Stainless
Tube: 1-1/2" O.D - 0.065" THK.
Length: 4.938"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 1.420 lbs