Flange Size: DN16 CF 34mm | 1.33" (1 1/3") OD Mini CF
Material: 316L Stainless Steel
Reference Number: BDA-133-ASME
Temperature Range: Bakeable to 450oC
Vacuum Series: Ultra High Vacuum (UHV)
Weight: 0.750 (lbs)
Rupture disk / safety pressure disc delivers reliable, consistent overpressure rupture protection
Pressure relief range: 9 to 11.5 psig
Ultra high vacuum (UHV) compatible all metal construction
Protection of systems with hazardous gases
Leak tight to 2 x 10-10 std. cc/sec of Helium
316L stainless steel body and disk membrane
Calculated flow rates: 107 SCFM on DN16CF 34mm | 1.33" (1-1/3 inch) OD ConFlat flange assembly