Flange 1: DN 50 ISO-KF
Flange 2: 2" OD Tube
Type: Half Nipple
Material: 304 Stainless Steel
Overall length: 3.225"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 0.610 lbs