Flange Size: DN 16 ISO-KF
Type: Flexible Bellows Hose
Overall length: 9.840"
Hose Material: 316 or 321 stainless steel
Flange material: 304 Stainless Steel
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C