Flange 1: DN 40 CF (2.75" OD)
Flange 2: DN 16 ISO-KF
Type: Straight Reducer
Material: 304 Stainless Steel
Overall length: 2.00"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 · 10-13 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -200 °C to 450 °C
Weight: 0.790 lbs