Flange 1: DN 25 ISO-KF
Tube OD 1: 1"
Type: Conical Reducer
Material: 304 Stainless
Flange 2: DN 16 ISO-KF
Tube OD 2: 3/4"
Overall length: 2.05"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 0.190 lbs