Flange Size: NW250 ISO-LF
Type: Flexible Coupling
Bellows O.D: 10.0"
Free Length: 11.22"
Wall Thickness: 0.012"
Flange & Cuff Material: 304 Stainless Steel
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 13.52 lbs