Tube OD: 6"
Flange type: DN 160 ISO-K
Elbow Type: Miter 90 Degree
Material: 304 Stainless Steel
Port Length: 6.06"
Wall Thickness: 0.120"
Finish: Bead Blast
Vacuum Range: 1 X 10-10 mbar to 1 bar
Temperature Range: -200 °C to 450 °C
Weight: 10.48 lbs