Adapter Type: Conical Reducer
Flange 1: DN 50 ISO-KF
Flange 2: DN 100 ISO-K
Material: 304 Stainless Steel
Tube OD 1: 2"
Tube OD 2: 4"
Port Length: 4.095"
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 1.940 lbs