Flange Size: DN 200 ISO-LF
Type: Blank
Material: 304 Stainless
Thickness: 0.630"
Bolt Circle: 10.240"
Bolt Hole Diameter: 0.437"
# Bolt Holes: 12
Vacuum Range: FKM: 1 X 10-8 mbar to 1 bar
Metal seal: 1 X 10-10 mbar to 1 bar
Temperature Range: FKM: -20 °C to 180 °C
Metal seal: -270 °C to 150 °C
Weight: 17.47 lbs